Thorlabs PDXC Piezo Inertia Stage Controller - Firmware Changelog 

This firmware is a device internal program for the PDXC Piezo Inertia Stage Controller. For installation instructions consult the user guide. 

Changelog
07-02-2021	Release V1.0

09-15-2021	V1.25
- Added output amplitude adjustment per direction in SMC mode
- New stages support

07-14-2022        V1.27
- Add analog In mode in open loop in D-Sub mode and SMC mode, when the input range of analog In signal is from 1V to 10V, representing with output forward amplitude 10% to 100% with 1x for Gain and 0 for offset, when the input range of analog In signal is from -1V to -10V, representing with output backward amplitude 10% to 100% with 1x for Gain and 0 for offset. The type of trigger edge to start the conversion can also be defined.
- Support the D-Sub stage without encoder
- Support 3-Axis USB joysticks
- Config the knob of joystick in Daisy-Chain mode

09-27-2022        V1.28
- Improve PD2 stage movement below 10Khz
- Fixed  the waveform output bug in SMC CH1