{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Calculator","Specifications"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Calculator","index":0,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[[3,12,3,13],[4,12,4,13],[5,12,5,13],[6,12,6,13],[1,3,1,7],[2,3,2,5],[2,6,2,7],[1,9,1,13],[2,12,2,13],[2,9,2,11],[6,9,6,11],[5,9,5,11],[2,1,7,1],[8,9,8,11],[3,3,3,5],[3,6,3,7],[4,3,4,5],[4,6,4,7],[5,3,5,5],[5,6,5,7],[6,3,6,5],[6,6,6,7],[7,3,7,5],[7,6,7,7],[8,3,8,5],[3,9,3,11],[4,9,4,11],[7,9,7,11],[9,9,9,11],[9,12,9,13],[8,6,8,7],[8,12,8,13],[7,12,7,13]]}
[]
[null,null,null,"Coupling Parameters",null,null,null,null,null,"Compatible Fiberport"]
[null,"This calculator can be used to find the best FiberPort for coupling based on your system setup.\n\nFor more information, please visit: \nhttps://www.thorlabs.com/FiberPorts",null,"Lens Type: ",null,null,null,null,null,"Item Number "]
[null,null,null,"Fiber Type: ",null,null,null,null,null,"Lens Type"]
[null,null,null,"Wavelength (nm): ",null,null,null,null,null,"Lower Coating Range (nm)"]
[null,null,null,"Connector Type: ",null,null,null,null,null,"Upper Coating Range (nm)"]
[null,null,null,"Beam Diameter (mm): ",null,null,null,null,null,"Connector Bulkhead"]
[null,null,null,"Mode Field Diameter (µm): ",null,null,null,null,null,"Focal Length (mm)"]
[null,null,null,"Calculated EFL (mm): ",null,null,null,null,null,"Lens NA"]
[null,null,null,null,null,null,null,null,null,"Lens CA (mm)"]

{"sheet":"Specifications","index":1,"n_rows":53,"n_cols":12,"rows_kept":53,"cut":false,"hidden":true,"merged":[]}
["Item number","Lens Type","Connector Type","EFL","Coating Lower","Coating Upper","Waist (mm)","NA","CA"]
["PAF2-2A","Aspheric","FC",2,350,700,0.33,0.5,2,null,"Application",1]
["PAF2-2B","Aspheric","FC",2,600,1050,0.43,0.5,2,null,"Input Lens ",1]
["PAF2-2C","Aspheric","FC",2,1050,1620,0.38,0.5,2,null,"Output Lens",1]
["PAF2-4E","Aspheric","FC",4,2000,5000,1.17,0.56000000000000005,5,null,"Input Fiber",1]
["PAF2-5A","Aspheric","FC",4.5999999999999996,350,700,0.75,0.53,4.9000000000000004,null,"Output Fiber",1]
["PAF2-5B","Aspheric","FC",4.5999999999999996,600,1050,1,0.53,4.9000000000000004,null,"Input Connector",1]
["PAF2-5C","Aspheric","FC",4.5999999999999996,1050,1620,0.87,0.53,4.9000000000000004,null,"Output Connector",1]
["PAF2-5D","Aspheric","FC",4.5999999999999996,1800,2400,0.9,0.53,4.9000000000000004]
["PAF2-7A","Aspheric","FC",7.5,350,700,1.23,0.3,4.5]
["PAF2-7B","Aspheric","FC",7.5,600,1050,1.62,0.3,4.5]
["PAF2-7C","Aspheric","FC",7.5,1050,1620,1.42,0.3,4.5]
["PAF2A-11A","Aspheric","FC/APC",11,350,700,1.8,0.2,4.4000000000000004,null,"Input Lens","Output Lens"]
["PAF2A-11B","Aspheric","FC/APC",11,600,1050,2.38,0.2,4.4000000000000004,null,"Aspheric","Aspheric"]
["PAF2A-11C","Aspheric","FC/APC",11,1050,1620,2.09,0.2,4.4000000000000004,null,"Achromatic","Achromatic"]
["PAF2A-11D","Aspheric","FC/APC",11,1800,2400,2.15,0.2,4.4000000000000004]
["PAF2A-15A","Aspheric","FC/APC",15.3,350,700,2.5,0.16,5,null,"Input Fiber","Output Fiber"]
["PAF2A-15B","Aspheric","FC/APC",15.3,600,1050,3.31,0.16,5,null,"Single Mode","Single Mode"]
["PAF2A-15C","Aspheric","FC/APC",15.3,1050,1620,2.9,0.16,5,null,"Multimode","Multimode"]
["PAF2A-15D","Aspheric","FC/APC",15.3,1800,2400,2.99,0.16,5,null,"Polarization Maintaining","Polarization Maintaining"]
["PAF2A-18A","Aspheric","FC/APC",18.399999999999999,350,700,3.01,0.15,5.5]
["PAF2A-18B","Aspheric","FC/APC",18.399999999999999,600,1050,3.98,0.15,5.5,null,"Input Connector","Output Connector"]
["PAF2A-18C","Aspheric","FC/APC",18.399999999999999,1050,1620,3.49,0.15,5.5,null,"FC/PC","FC/PC"]
["PAF2A-18D","Aspheric","FC/APC",18.399999999999999,1800,2400,3.6,0.15,5.5,null,"FC/APC","FC/APC"]
["PAF2-A4A","Achromatic","FC",4,350,700,0.65,0.22,1.8,null,"FC/PC or FC/APC","FC/PC or FC/APC"]
["PAF2-A4B","Achromatic","FC",4,600,1050,0.87,0.22,1.8,null,"SMA","SMA"]
["PAF2-A4C","Achromatic","FC",4,1050,1620,0.76,0.22,1.8]
["PAF2P-11A","Aspheric","FC/PC",11,350,700,1.8,0.2,4.4000000000000004]
["PAF2P-11B","Aspheric","FC/PC",11,600,1050,2.38,0.2,4.4000000000000004]
["PAF2P-11C","Aspheric","FC/PC",11,1050,1620,2.09,0.2,4.4000000000000004]
["PAF2P-11D","Aspheric","FC/PC",11,1800,2400,2.15,0.2,4.4000000000000004]
["PAF2P-11E","Aspheric","FC/PC",11,2000,5000,3.21,0.18,4]
["PAF2P-15A","Aspheric","FC/PC",15.3,350,700,2.5,0.16,5]
["PAF2P-15B","Aspheric","FC/PC",15.3,600,1050,3.31,0.16,5]
["PAF2P-15C","Aspheric","FC/PC",15.3,1050,1620,2.9,0.16,5]
["PAF2P-15D","Aspheric","FC/PC",15.3,1800,2400,2.99,0.16,5]
["PAF2P-18A","Aspheric","FC/PC",18.399999999999999,350,700,3.01,0.15,5.5]
["PAF2P-18B","Aspheric","FC/PC",18.399999999999999,600,1050,3.98,0.15,5.5]
["PAF2P-18C","Aspheric","FC/PC",18.399999999999999,1050,1620,3.49,0.15,5.5]
["PAF2P-18D","Aspheric","FC/PC",18.399999999999999,1800,2400,3.6,0.15,5.5]
["PAF2S-11A","Aspheric","SMA",11,350,700,1.8,0.2,4.4000000000000004]
["PAF2S-11B","Aspheric","SMA",11,600,1050,2.38,0.2,4.4000000000000004]
["PAF2S-11C","Aspheric","SMA",11,1050,1620,2.09,0.2,4.4000000000000004]
["PAF2S-11D","Aspheric","SMA",11,1800,2400,2.15,0.2,4.4000000000000004]
["PAF2S-11E","Aspheric","SMA",11,2000,5000,3.21,0.18,4]
["PAF2S-4E","Aspheric","SMA",4,2000,5000,1.17,0.56000000000000005,5]
["PAF2S-5A","Aspheric","SMA",4.5999999999999996,350,700,0.75,0.53,4.9000000000000004]
["PAF2S-5B","Aspheric","SMA",4.5999999999999996,600,1050,1,0.53,4.9000000000000004]
["PAF2S-5C","Aspheric","SMA",4.5999999999999996,1050,1620,0.87,0.53,4.9000000000000004]
["PAF2S-5D","Aspheric","SMA",4.5999999999999996,1800,2400,0.9,0.53,4.9000000000000004]
["PAF2S-7A","Aspheric","SMA",7.5,350,700,1.23,0.3,4.5]
["PAF2S-7B","Aspheric","SMA",7.5,600,1050,1.62,0.3,4.5]
["PAF2S-7C","Aspheric","SMA",7.5,1050,1620,1.2,0.3,4.5]