Thorlabs Optical Power Monitor Application + TLPM Instrument Driver - Readme
The Thorlabs Optical Power Monitor Application is used to operate the following Thorlabs Powermeters :
PM160x, PM16-series, PM400, PM100D, PM100A, PM100USB and PM200.

The TLPM driver installs to into your system's VXIPnP directory. This is typically 'C:\Program Files\IVI Foundation\VISA\WinNT' or '\C:\VXIPNP\WinNT'. The instrument driver package was created with MinGW32 V-4.8.1 and MinGW64 V-4.7.1.The LabVIEW version of this driver was generated with LabVIEW Interface Generator for LabWindows/CVI Instrument Drivers 2.0 in conjunction with LabVIEW 8.5. The .NET managed library was generated by the National Instruments Measurement Studio plug-in for Visual Studio.NET 2015.

Note:
This software comes with additional software packages:
	- MS .Net Framework		http://www.microsoft.com/net
	- Infragistics WPF Controls	http://www.infragistics.com

License:
The Optical Power Monitor Application software is copyright Ó 2018, Thorlabs GmbH. For license details please see file License.rtf in the applications installation directory.
The TLPM instrument driver libraries are copyright Ó 2018, Thorlabs GmbH.

Supported Platforms:
This software was verified with the following platforms:
	- Windows 7 (SP1+)	32-bit and 64-bit version
	- Windows 8.1		32-bit and 64-bit version
 	- Windows 10         	32-bit and 64-bit version

Optical Power Monitor Application Change log:
V1.0	March-2018	Initial Release

TLPM VXIpnp Instrument Driver Changelog:
V4.1	March-2018	Initial Release