Thorlabs PDXC- Readme 
Use this software to operate Piezo Stage Controller (PDXC).

Note:
This software comes with additional software packages:
1. Microsoft .Net Framework 4.6.2 Full Profile or higher version is required. It is included on the CD. If installing from the web, the install program will check and download it from internet if necessary. 

License:
This software is copyright ©2021-2023, Thorlabs Shanghai. For license details please see file Thorlabs End-user License.rtf.

Supported platforms:                                                                                                                                                                                         
This software was verified with the following platforms:
 - Windows® 7 SP1 updated with KB3020369 and KB3125574 (32-bit and 64-bit Operating System)
 - Windows® 10 (32-bit and 64-bit version Operating System)
 - Windows® 11

Additional Software
Microsoft .Net Framework 4.6.2 Full Profile or higher version is required. The install program will check and download it from the internet if necessary.

Changelog

May-20-2021 - Release V1.1.1
   First release

Sept-13-2021 - Release V1.2.0
   Support to adjust the amplitude of driving waveforms for the two directions separately, hence allow for fine tuning of speed.

Jul-26-2022 - Release V1.4.1
1.	Add Analog In mode in Open Loop in D-Sub mode and SMC mode.
2.	Add joystick support in Daisy-Chain mode.

May-24-2023 - Release V1.5.2
1.	Verify compatibility with Windows® 11.
2.	Added support for PDXR1(/M)

Aug-14-2023 - Release V1.6.0
1.	Add save/load configuration function.
2.	Expand Analog in Gain range for PDXR1.
3.	Set PID Kd parameter limit>=0