Thorlabs DC2100 – High Power LED Driver -  VISA Instrument Driver - Readme

This instrument driver library provides programming support for the Thorlabs DC2100 – High Power LED Driver.

The instrument driver package was created with National Instruments LabWindows/CVI 8.5. The LabVIEW version of this driver was generated converting the CVI version with NI-LabVIEW 8.5. A convenient way to import the driver directly to your NI-LabView environment is to use the NI-LabView 'Import CVI Instrument Driver'  functionality.

Important Note 
This driver needs a NI-VISA engine to be installed. You may download a VISA engine from http://www.ni.com/visa.

License
For license details please see file License.rtf.

Changelog
Mar-26-2009	Initial Release

Apr-18-2013 Release 2.0
	- driver is VXIpnp compatible for easier Matlab import
	- 64 bit version of the driver
	- .Net Wrapper for 64 bit

Mar-28-2014 Release 2.1
	- usb driver updated to version 2.08.30 with blue screen bug fix