Readme - Thorlabs DC4100 Series- Four Channel LED Driver

Use this software to control a DC4100 Series - Four Channel LED Driver remotely from your PC.

Important Note

This software needs a NI-VISA engine to be installed. It will be installed automatically if your PC does not have a compatible version installed.

License

For license details please see file License.rtf.

Changelog

Apr-01-2009 - Initial Release 1.0

Oct-01-2009 - Release V1.1

Jan-10-2011	Release V1.2 with Driver for Windows 64 bit

Mar-15-2012	Release V2.0 
	- supports DC4104 instrument
	- new LabView Sample

Feb-25-2014 Release V2.1
	- C++ Sample added to operate the DC4100 series instrument
	- .Net Sample added to operate the DC4100 series instrument
	- driver function description added.
	- Sample for LabView 8.5 updated
	- LabView llb with sample for LabView 2009 (64 bit) added to the installation package

Mar-28-2014 Release V2.2
	- usb driver updated to version 2.08.30

Oct-04-2024 Release V2.3
	- usb driver updated to version 2.12.36