Thorlabs PM320E Datalog - Readme

This tool can be used to sample, display, and store power or energy reading data from the THORLABS PM320E and PM300E dual channel optical Power/Energy Meters.
The PM320E / PM300E device communicates to the PC via USB link. To run the program it is not necessary to install the VISA instrument drivers from the CD.
To achieve highest data rates with one power sensor it is recommended to disable the unused channel.

Important Note: 
This driver needs a NI-VISA runtime engine to be installed. You may download the software from http://www.ni.com/visa.

License
For license details please see file License.rtf.

Changelog
Jul-29-2009	Release V1.0